2.

a. DCW places the 16-bit half-word into memory. This is useful because it allows us to assist and control the assembly process. In this case this is helpful in storing large expressions into memory for us to call and use later, even if a certain execution requires more space to run than is available in the registers.

b.